



Reliant Floor Case Collection (2074, 2075, 2076, 2174, 2175, 2176)



|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| W/ Cornice | “A” | “B” | “C” |  | “A” | “B” | “C” |
| 2174XX-XX-XX | 48” | 80” | 16” | 2074XX-XX-XX | 48” | 72” | 16” |
| 2175XX-XX-XX | 60” | 80” | 16” | 2075XX-XX-XX | 60” | 72” | 16” |
| 2176XX-XX-XX | 72” | 80” | 16” | 2076XX-XX-XX | 72” | 72” | 16” |

Shelving:



* 4 Half-Size Shelves
  + 4’ Shelf Dimensions: 23 ”x 13 ” x ¼”
  + 5’ Shelf Dimensions: 29 ½”x 14” x ¼”
  + 6’ Shelf Dimensions: 35 ½”x 14” x ¼”
* The case utilizes a standard for shelf adjustments in 1” increments.
* Each shelf has a capacity of 25 lbs.

Doors:

* Sliding doors that open from both sides for easy access. Door handles

Come in bronze or satin to match the case.

* Lock mechanism is the Selby-033 cam lock that comes with 2 keys.

Lighting:

* Lighted units come with LED strip lights with a 10’ cord and case-mounted

on/off switch.

Materials:

* Case frame is made of anodized aluminum in a variety of colors.
* Cases are available with a variety of back options including custom printed options.

Assembly/Weight/Shipping:

* Cases arrive semi-assembled. Installers will need to unpack/untape the unit, install the shelves, install the door handles, and level the case. Tip protection is also provided and must be installed to meet furniture tip over requirements.
* Cases vary from 275 to 500 lbs.
* Cases will arrive on a pallet shrink-wrapped and packaged for safe arrival.